{"text_format":"3","workbook":"xls","n_sheets":1,"sheets":["底价单"],"not_rendered":{"external_links":1,"defined_names":2},"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"底价单","index":0,"n_rows":68,"n_cols":7,"rows_kept":68,"merged":[[0,0,0,6],[1,0,1,6],[2,0,2,2],[3,0,3,4],[3,5,3,6],[17,1,17,6],[20,0,20,6],[21,1,21,6],[22,1,22,6],[23,1,23,6],[24,1,24,6],[25,1,25,6],[26,1,26,6],[27,1,27,6],[28,1,28,6],[29,1,29,6],[30,1,30,6],[31,1,31,6],[32,1,32,6],[33,1,33,6],[34,1,34,6],[35,1,35,6],[36,1,36,6],[38,1,38,6],[39,1,39,6],[40,1,40,6]],"flags":["formulas_cached_only"]}
["湖北亚东水泥有限公司"]
["估  价  单"]
["工作单号：A201900336"]
[" 工程名称：生活区宿舍应急照明灯及安全出口灯配电等工作",{"$nulls":4},"   日期 ：2019年  11月6日"]
["项目","名             称","数量","单位","单价","总价","备  注"]
[1,"承包商自备材料费",1,"式"]
[]
[2,"承包商施工工资",1,"式"]
[]
[3,"安全施工费",1,"式"]
[]
[4,"管理费",1,"式"]
[]
[5,"捐税",1,"式"]
[]
[]
[null,"工程含税价   3  %合计",{"$nulls":4},"增值税计含税价，普票不计"]
[null,"工程底价：人民币          万         仟         佰            拾           元整"]
[]
[]
["施工说明："]
[null,"1.本工作范围及要求如下："]
[null,"（1） 生活区宿舍应急照明灯及安全出口灯电源敷设及灯具更换安装"]
[null,"①为满足相关法律要求，现从生活区配电室拉电源至每栋楼，每栋安全出口灯及应急灯重新配置电源"]
[null,"②配置的电源为双电源，开关在生活区配电室，和生活区消防泵为同级电源（该电源一组是市电，一"]
[null,"组为水厂发电机供电）"]
[null,"（2） 福利中心部分坏掉的应急照明灯及安全出口灯更换"]
[null,"2.需按照监工指定地点接电源，管线需按照要求进行配置，桥架内电缆需绑扎好。开关箱安装完毕后"]
[null,"焊接处需进行喷漆处理"]
[null,"3.除由业主供给的材料外，其它一般消耗性材料及所有施工机具均由承包商自理，并按照监工要求认"]
[null," 真配合施工。"]
[null,"4.本工作系总价包干方式,议价前由业主承办人现场讲解施工程序及工作范围,承包商如有疑问应及提出，"]
[null,"一经决标后不得有任何异议。"]
[null,"5.承包商于施工过程中务必加强安全管理，采取各项安全防护措施，配备各种安全警戒标志，若不幸发"]
[null,"  生任何安全意外等工安事故，导致人员伤亡或导致社会上之不良影响，皆由承包商自行负责，概与业"]
[null,"  主无涉，若业主因此受到损失，亦须由承包商负责赔偿。"]
[null,"6.在施工中有疑问,承包商需与监工进行协商处理,承包商擅自主张造成损失由包商负责,不得有异议"]
[null,"7.承包商应维持施工范围内的整洁,每天下班前将施工的废料等带走,将环境整理干净后才可离开"]
[null,"8.无条件配合本公司监工人员对现场不合理部分进行修改,承包商不得有任何异议"]
[null,"9.工作完成后必须配合本公司监工进行相关测试,经本公司监工人员确认后工作才算完工"]
[null,"10.本工程经验收合格后，工程款一次付清。"]
["一","承包商施工材料费"]
[1,"松下86型5孔插座（AC220V  10A",130,"PC"]
[2,"正大天虹镀锌铁管20Φ",760,"M"]
[3,"镀锌开关箱400*300*150",1,"ST"]
[4,"20Φ镀锌线管接线盒（三通或四通盒）",30,"PC"]
[5,"86明装镀锌铁底盒",130,"PC"]
[6,"加厚型20Φ金属软管",40,"M"]
[7,"加厚型20Φ金属软管接头",160,"PC"]
[8,"20Φ固定用镀锌发卡（厚度2毫米）",400,"PC"]
["二","承包商施工工资"]
[1,"各式电缆敷设工作",1300,"M"]
["2","插座安装固定及接线工作",130,"ST"]
["3","镀锌铁管及软管安装固定工作（需根据现场情况进行固定安装，含铁管切割及绞牙固定软管等）"]
[null,null,800,"M"]
[4,"开关箱安装固定及箱内设备接线等工作",1,"ST"]
[5,"A1栋混凝土地面开孔走线管及复原等工作（比照生活区消防水管进行开孔）"]
[null,null,5,"PC"]
[6,"三通或四通盒安装固定及接线工作（含固定所需材料费）"]
[null,null,30,"ST"]
[7,"电缆沟盖板掀开及整理工作（部分盖板上方土方需清理）"]
[null,null,80,"M"]
[8,"安全出口标示牌及应急照明灯安装固定及接线工作"]
[null,null,125,"PC",null,null,"含固定所需材料费"]
[9,"坏掉的应急照明灯及安全出口灯更换工作（一拆一装，因固定尺寸不同，需重新打孔固定）"]
[null,null,34,"PC"]
[10,"墙面开孔及复原工作",6,"PC"]
[11,"地面开挖及复原工作（预埋深度为30CM以上）",30,"M"]